                  STATIONS Table Layout for Rivendell

The STATIONS table contains data about each workstation in the system.
Following is the layout of a record in the SERVICES table:

FIELD NAME           TYPE               REMARKS
---------------------------------------------------------------
NAME                 char(64)           Primary Key
DESCRIPTION          char(64)           Indexed
USER_NAME            char(255)          Current User
DEFAULT_NAME         char(255)          Default User
IPV4_ADDRESS	     char(15)
TIME_OFFSET          int(11)
BACKUP_DIR           char(255)
BACKUP_LIFE          int(11)
BROADCAST_SECURITY   int(10) unsigned   0=HostSec, 1=UserSec
HEARTBEAT_CART       int(10) unsigned
HEARTBEAT_INTERVAL   int(10) unsigned
STARTUP_CART         int(10) unsigned
EDITOR_PATH          char(255)
FILTER_MODE          int(11)            0=Synchronous, 1=Asynchronous
SYSTEM_MAINT         enum('N','Y')
STATION_SCANNED      enum('N','Y')
HAVE_OGGENC          enum('N','Y')
HAVE_OGG123          enum('N','Y')
HAVE_FLAC            enum('N','Y')
HAVE_LAME            enum('N','Y')
HAVE_MPG321          enum('N','Y')
HPI_VERSION          char(16)
JACK_VERSION         char(16)
ALSA_VERSION         char(16)
CARD0_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD0_NAME           char(64)
CARD0_INPUTS         int(11) signed
CARD0_OUTPUTS        int(11) signed
CARD1_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD1_NAME           char(64)
CARD1_INPUTS         int(11) signed
CARD1_OUTPUTS        int(11) signed
CARD2_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD2_NAME           char(64)
CARD2_INPUTS         int(11) signed
CARD2_OUTPUTS        int(11) signed
CARD3_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD3_NAME           char(64)
CARD3_INPUTS         int(11) signed
CARD3_OUTPUTS        int(11) signed
CARD4_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD4_NAME           char(64)
CARD4_INPUTS         int(11) signed
CARD4_OUTPUTS        int(11) signed
CARD5_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD5_NAME           char(64)
CARD5_INPUTS         int(11) signed
CARD5_OUTPUTS        int(11) signed
CARD6_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD6_NAME           char(64)
CARD6_INPUTS         int(11) signed
CARD6_OUTPUTS        int(11) signed
CARD7_DRIVER         int(11) signed     0=None, 1=Hpi, 2=Jack, 3=ALSA
CARD7_NAME           char(64)
CARD7_INPUTS         int(11) signed
CARD7_OUTPUTS        int(11) signed
