               RECORDINGS Table Layout for Rivendell

The RECORDINGS table holds data concerning each individual automatic
recording programmed on the system.  Following is the layout of a
record in the RECORDINGS table:

FIELD NAME           TYPE              REMARKS
------------------------------------------------------------------
ID                   int(10) unsigned  Primary key, auto increment
IS_ACTIVE            enum('N','Y')
TYPE                 int(11)           0=Recording,1=Macro Event,
                                       2=Switch Event,3=Playout,
                                       4=Download,5=Upload
STATION_NAME         char(64)          From STATIONS.NAME
CHANNEL              int(10) unsigned
CUT_NAME             char(12)          From CUTS.CUT_NAME
SUN                  enum('N','Y')
MON                  enum('N','Y')
TUE                  enum('N','Y')
WED                  enum('N','Y')
THU                  enum('N','Y')
FRI                  enum('N','Y')
SAT                  enum('N','Y')
DESCRIPTION          char(64)          Remarks

START_TYPE           int(10)           0=Hard Timed,1=GPI
START_TIME           time
START_LENGTH         int(11)
START_MATRIX         int(11)           from MATRICES.MATRIX
START_LINE           int(11)
START_OFFSET         int(11)
END_TYPE             int(10)           0=Hard Timed,1=GPI,2=Length
END_TIME             time
END_LENGTH           int(11)
END_MATRIX           int(11)           from MATRICES.MATRIX
END_LINE             int(11)

LENGTH               int(10) unsigned  in milliseconds
START_GPI            int(11) signed    -1 = None
END_GPI              int(11) signed    -1 = None
ALLOW_MULT_RECS      enum('N','Y')
MAX_GPI_REC_LENGTH   int(10) unsigned
TRIM_THRESHOLD       int(11)           in 1/100 dBFS
NORMALIZE_LEVEL      int(11)           in 1/100 dBFS
STARTDATE_OFFSET     int(10) unsigned
ENDDATE_OFFSET	     int(10) unsigned
EVENTDATE_OFFSET     int(11)
FORMAT               int(11) signed    0 = PCM16, 2 = Layer 2, 3 = Layer 3
CHANNELS             int(11) signed
SAMPRATE             int(11) signed
BITRATE              int(11) signed
QUALITY              int(11) signed
MACRO_CART	     int(10) unsigned
SWITCH_INPUT         int(11)
SWITCH_OUTPUT        int(11)
EXIT_CODE            int(11)           0 = Ok, 1 = Short Length, 
                                       2 = Low Level, 3 = High Level
ONE_SHOT             enum ('N','Y')
URL                  char(255)
URL_USERNAME         char(64)
URL_PASSWORD         char(64)
FEED_ID              int               From FEEDS.ID
