                   DECKS Table Layout for Rivendell

The DECKS table holds data concerning each configured netcatcher
recording interface on the system.  Following is the layout of a
record in the DECKS table:

FIELD NAME           TYPE              REMARKS
------------------------------------------------------------------
ID                   int(10) unsigned  Primary key, auto increment
STATION_NAME         char(64)          From STATIONS.NAME
CHANNEL              int(10) unsigned  0 = Audition Channel
CARD_NUMBER          int(11) signed    -1 = None Assigned
STREAM_NUMBER        int(11) signed    -1 = None Assigned
PORT_NUMBER          int(11) signed    -1 = None Assigned
PORT_TYPE            enum('A','D')     A = Analog, D= Digital
MON_PORT_NUMBER      int(11) signed
DEFAULT_MONITOR_ON   enum('N','Y')
DEFAULT_FORMAT       int(10) signed
DEFAULT_CHANNELS     int(10) signed
DEFAULT_SAMPRATE     int(10) signed    RETIRED
DEFAULT_BITRATE      int(10) signed
DEFAULT_THRESHOLD    int(10) signed
SWITCH_STATION       char(64)          From OUTPUTS.STATION_NAME
SWITCH_MATRIX        int(11)           From OUTPUTS.MATRIX
SWITCH_OUTPUT        int(11)           From OUTPUTS.NUMBER
SWITCH_DELAY         int(10) unsigned
