B.2. BroadcastTools 10x1
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.2. BroadcastTools 10x1

Driver Name:

  BroadcastTools 10x1

Supported RML Commands:

  Switch Take ['ST']

Control is done by means of an RS-232C connection to a four pin RJ11 modular jack on the back of the unit (an adapter to a standard DB9 connector is supplied by Broadcast Tools with the unit). Serial port parameters should be set to 2400 baud rate, no parity, 8 data bits, 1 stop bit, CR/LF termination.

Prev | Up | Next
Appendix B. Supported GPIO/Switcher Devices | Home | B.3. BroadcastTools 16x1