B.4. BroadcastTools 16x2
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.4. BroadcastTools 16x2

Driver Name:

  BroadcastTools 16x2

Supported RML Commands:

  GPO Set ['GO']
  Switch Take ['ST']

Control is done by means of an RS-232C connection to a four pin RJ11 modular jack on the back of the unit (an adapter to a standard DB9 connector is supplied by Broadcast Tools with the unit). Serial port parameters should be set to 9600 baud rate, no parity, 8 data bits, 1 stop bit, CR/LF termination.

Operation in 'multidrop' mode is not supported.

Prev | Up | Next
B.3. BroadcastTools 16x1 | Home | B.5. BroadcastTools 8x2