B.28. Ross NK Video Switchers (via SCP/A Serial Interface)
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.28. Ross NK Video Switchers (via SCP/A Serial Interface)

Driver Name:

  Ross NK-SCP/A Interface

Supported RML Commands:

  Switch Take ['ST']

Control is done by means of an RS-232C connection to a NK-SCP/A serial interface. Serial port parameters should be set to 9600 baud rate, no parity, 8 data bits, 1 stop bit, CR termination. The Breakaway to use is defined by setting the 'Card' parameter in the driver configuration, with Card 0 = Breakaway 1, Card 1 = Breakaway 2, etc.

Prev | Up | Next
B.27. Quartz Electronics Type 1 Routing Protocol | Home | B.29. Serial Port Modem Control Lines