B.9. BroadcastTools Sentinel 4 Web AES Switcher
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.9. BroadcastTools Sentinel 4 Web AES Switcher

Driver Name:

  BroadcastTools Sentinel 4 Web

Supported RML Commands:

  Switch Take ['ST']

Control is done by means of a TCP/IP connection to the unit's integrated Ethernet port.

On the `Email/Network Setup` page of the unit, be sure that the `TCP Enabled` box is checked and that `TCP Listen Port` is set to the same number as is used in the `IP Port` setting in Rivendell's driver configuration (`56` by default).

Prev | Up | Next
B.8. BroadcastTools GPI-16 General Purpose Input Module | Home | B.10. BroadcastTools SRC-16