B.20. Livewire LWRP Audio
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.20. Livewire LWRP Audio

Driver Name:

  Livewire LWRP Audio

Supported RML Commands:

  Switch Take ['ST']

Livewire is a distributed audio router and control system, with the components (called 'nodes') configured and controled via TCP/IP. More information can be found at http://www.axiaaudio.com/.

This driver can be used to create and remove connections between audio sources and destinations via Livewire Routing Protocol (LWRP).

Configuration is a matter of entering the IP address, password and base output number for each node in `RDAdmin->ManageHosts->Switcher/GPIO->LivewireNodes`. The driver will autodetect all other parameters from the nodes themselves. The resulting constellation of nodes can be controled with the 'Switch Take' ['ST'] RML by specifying the Livewire source stream number as the `input` parameter and the the base output number+the slot number-1 for the `output` parameter.

Prev | Up | Next
B.19. Kernel GPIO | Home | B.21. Livewire LWRP GPIO