B.36. Software Authority Protocol
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.36. Software Authority Protocol

Driver Name:

  Software Authority Protocol

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']
  GPO Set ['GO']
  Switch Take ['ST']

Used to control devices (such as the Axia 'PathFinder' system) by means of the 'Software Authority' protocol. Control is by means of a TCP/IP connection (typically to port 9500) on the controled system. The `Card` parameter should be set to the 'Router Number' of the router to be controlled.

Most parameters, including the number of inputs and outputs as well as the endpoint names, are autodetected by the driver.

Prev | Up | Next
B.35. Sine Systems ACU-1 (Prophet Version) | Home | B.37. Starguide III Satellite Receiver