B.40. Wheatnet Blade SLIO
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.40. Wheatnet Blade SLIO

Driver Name:

  WheatNet SLIO

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']
  GPO Set ['GO']

Control is done by means of a TCP/IP connection to port 55776 on a blade. The only required configuration parameters are `IP Address` and `IP Port`. The number of pins is auto-detected at driver startup.

Prev | Up | Next
B.39. Wheatnet Blade LIO | Home | Appendix C. Filepath Wildcards