B.8. BroadcastTools GPI-16 General Purpose Input Module
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.8. BroadcastTools GPI-16 General Purpose Input Module

Driver Name:

  BroadcastTools GPI-16

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']

Control is done by means of a serial connection to the unit's integrated serial port. There is also a 'plus' version that features an integrated type B USB interface that simulates a serial port.

The unit should work correctly with factory default settings. The Rivendell serial interface should be set to use 9600 bits/sec, 8 bits, 1 stop bit and no flow control.

Prev | Up | Next
B.7. BroadcastTools ADMS 44.22 Analog/AES Digital Matrix Switcher | Home | B.9. BroadcastTools Sentinel 4 Web AES Switcher