B.18. Harlond Virtual Mixer
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.18. Harlond Virtual Mixer

Driver Name:

  Harlond Virtual Mixer

Supported RML Commands:

  Fire Salvo ['FS']
  GPI Enable ['GE']
  GPI Set ['GI']
  GPO Set ['GO']
  Switch Add ['SA']
  Switch Level ['SL']
  Switch Remove ['SR']
  Switch Take ['ST']

Control is by means of a TCP/IP connection to port 5002. Output busses are mapped as follows:

Table B.1. Harlond Output Buss Mappings

Output | Buss
--- | ---
1 | PGM
2 | AUD
3 | UTL
4 | CUE

Input channel ON/OFF is sensed/controlled by means of the respective GPIO number using GE/GI/GO RMLs.

Prev | Up | Next
B.17. BroadcastTools Universal 4.1MLR>>Web | Home | B.19. Kernel GPIO