<?xml version="1.0" encoding="ISO-8859-1"?>
<article xmlns="http://docbook.org/ns/docbook" version="5.0">
<info>
  <title>Rivendell RDCatch Monitor Protocol</title>
  <author>
    <personname>
      <firstname>Fred</firstname>
      <surname>Gleason</surname>
      <email>fredg@paravelsystems.com</email>
    </personname>
  </author>
</info>

<sect1 xml:id="overview">
  <title>Overview</title>
  <para>
    This defines the IP protocol used for communication between different
    modules of Rivendell and the
    <command>rdcatchd</command><manvolnum>8</manvolnum> daemon.
  </para>
  <para>
    Connection to ripcd is by means of a TCP SOCK_STREAM connection to TCP
    port <userinput>6006</userinput>. The format of a message is as follows:
  </para>
  <para>
    <replaceable>cmd-code</replaceable> [<replaceable>arg</replaceable>] [<replaceable>...</replaceable>]!
  </para>
  <variablelist>
    <varlistentry>
      <term>
	<replaceable>cmd-code</replaceable>
      </term>
      <listitem>
	<para>
	  A two letter command code, describing the generic action to be
	  performed
	</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term>
	<replaceable>arg</replaceable>
      </term>
      <listitem>
	<para>
	  Zero or more arguments, delimited by spaces or, if the last
	  argument, by ! (see below)
	</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term>
	!
      </term>
      <listitem>
	<para>
	  The ASCII character  33, indicating the end of the command sequence.
	</para>
      </listitem>
    </varlistentry>
  </variablelist>
</sect1>

<sect1 xml:id="sect.unprivileged_commands">
  <title>Unprivileged Commands</title>
  <para>
    No authentication is required to execute these.
  </para>
  <sect2 xml:id="sect.unprivileged_commands.drop_connection">
    <title>Drop Connection</title>
    <para>
      End the session and drop the TCP connection.
    </para>
    <para>
      <userinput>DC!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="sect.unprivileged_commands.send_password">
    <title>Send Password</title>
    <para>
      Send a password to the server for authentication.
    </para>
    <para>
      <userinput>PW <replaceable>passwd</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term>
	  <replaceable>passwd</replaceable>
	</term>
	<listitem>
	  A password to be supplied before granting the client access.
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      <command>rdcatchd</command><manvolnum>8</manvolnum> will respond
      with <computeroutput>PW +!</computeroutput> or
      <computeroutput>PW -!</computeroutput>, indicating the success or
      failure of the authentication.
    </para>
  </sect2>
</sect1>

<sect1 xml:id="sect.privileged_commands">
  <title>Privileged Commands</title>
  <para>
     A connection must be authenticated before these can be executed.
  </para>

  <sect2 xml:id="sect.privileged_commands.deck_event_processed">
    <title>Deck Event Processed</title>
    <para>
      Sent by RDCatchd whenever a deck event is processed.
    </para>
    <para>
      <userinput>DE <replaceable>deck-num</replaceable>
      <replaceable>event-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>deck-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the deck originating the event. Record decks have
	    numbers in the range <computeroutput>1</computeroutput> through
	    <computeroutput>127</computeroutput>, while Play decks have
	    numbers in the range <computeroutput>128</computeroutput> through
	    <computeroutput>254</computeroutput>.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>event-num</replaceable></term>
	<listitem>
	  <para>
	    The new event state of the specified deck.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      See <xref linkend="sect.privileged_commands.request_deck_status" /> for
      the list of possible deck event states.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.reload_deck_list">
    <title>Reload Deck List</title>
    <para>
      Reload the record/play deck configuration.
    </para>
    <para>
      <userinput>RD!</userinput>
    </para>
    <para>
      <command>rdcatchd</command><manvolnum>8</manvolnum> will respond with
      <computeroutput>RS +!</computeroutput>.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.reload_event_list">
    <title>Reload Event List</title>
    <para>
      Reload the list of scheduled events.
    </para>
    <para>
      <userinput>RS!</userinput>
    </para>
    <para>
      <command>rdcatchd</command><manvolnum>8</manvolnum> will respond with
      <computeroutput>RS +!</computeroutput>.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.add_event">
    <title>Add Event</title>
    <para>
      Add event to the event list.
    </para>
    <para>
      <userinput>RA <replaceable>event-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>event-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the event to add.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      <command>rdcatchd</command><manvolnum>8</manvolnum>
      will respond with
      <computeroutput>RA <replaceable>event-num</replaceable>+!</computeroutput>.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.remove_event">
    <title>Remove Event</title>
    <para>
      Remove event from the event list.
    </para>
    <para>
      <userinput>RR <replaceable>event-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>event-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the event to remove.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      <command>rdcatchd</command><manvolnum>8</manvolnum>
      will respond with
      <computeroutput>RR <replaceable>event-num</replaceable>+!</computeroutput>.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.update_event">
    <title>Update Event</title>
    <para>
      Update event from the event list.
    </para>
    <para>
      <userinput>RU <replaceable>event-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>event-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the event to update.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      <command>rdcatchd</command><manvolnum>8</manvolnum>
      will respond with
      <computeroutput>RU <replaceable>event-num</replaceable>+!</computeroutput>.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.request_deck_status">
    <title>Request Deck Status</title>
    <para>
      Request the current deck status.
    </para>
    <para>
      <userinput>RE <replaceable>deck-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>deck-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the deck for which to return status.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      If <replaceable>deck-num</replaceable> is greater than zero,
      <command>rdcatchd</command><manvolnum>8</manvolnum> will respond with 
      <computeroutput>RE <replaceable>deck-num</replaceable> 
      <replaceable>status</replaceable> <replaceable>id</replaceable>
      <replaceable>cutname</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>deck-num</replaceable></term>
	<listitem>
	  <para>
	    Channel number
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>status</replaceable></term>
	<listitem>
	  <para>
	    The current status of the deck. Possible values are:
	  </para>
	  <para>
	    <table frame="all">
	      <title>Deck Status Codes</title>
	      <tgroup cols="2" align="left" colsep="1" rowsep="1">
		<colspec colname="Code"  colwidth="1.0*" />
		<colspec colname="Meaning" colwidth="10.0*" />
		<thead>
		  <row><entry>Code</entry><entry>Meaning</entry></row>
		</thead>
		<tbody>
		  <row><entry>0</entry><entry>Offline</entry></row>
		  <row><entry>1</entry><entry>Idle</entry></row>
		  <row><entry>2</entry><entry>Ready</entry></row>
		  <row><entry>3</entry><entry>Active (playing or recording)</entry></row>
		  <row><entry>4</entry><entry>Waiting (for a GPI)</entry></row>
		</tbody>
	      </tgroup>
	    </table>
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>event-id</replaceable></term>
	<listitem>
	  <para>
	    ID number of current event (from RECORDINGS table)
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>cutname</replaceable></term>
	<listitem>
	  <para>
	    The cutname of the event (present only for
	    <replaceable>status</replaceable>==<computeroutput>3</computeroutput>).
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      If <replaceable>channel</replaceable> is zero,
      <command>rdcatchd</command><manvolnum>8</manvolnum> will respond for
      every event whose status is non-idle.
    </para>
    <para>
      An <computeroutput>RE</computeroutput> packet will also be sent
      automatically to all active connections upon any change of deck status.
    </para>
  </sect2>
  <sect2 xml:id="sect.privileged_commands.enable_metering">
    <title>Enable Metering</title>
    <para>
      Enable/Disable Audio Metering
    </para>
    <para>
      <userinput>RM <replaceable>state</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>state</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = Enabled,
	    <computeroutput>0</computeroutput> = Disabled.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      When metering is active, meter data packets will be periodically sent,
      as follows:
    </para>
    <para>
      <computeroutput>RM <replaceable>deck</replaceable>
      <replaceable>chan</replaceable>
      <replaceable>level</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>deck</replaceable></term>
	<listitem>
	  <para>
	    Deck number
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>chan</replaceable></term>
	<listitem>
	  <para>
	    Channel, <computeroutput>0</computeroutput> = Left,
	    <computeroutput>1</computeroutput> = Right
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>level</replaceable></term>
	<listitem>
	  <para>
	    Left audio level, in 1/100 of dbFS
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>
  
  <sect2 xml:id="sect.privileged_commands.stop_deck">
    <title>Stop Deck</title>
    <para>
      Stop active event.
    </para>
    <para>
      <userinput>SR <replaceable>deck-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>deck-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the deck to stop.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.purge_event">
    <title>Purge Event</title>
    <para>
      Report purging of one-shot event.
    </para>
    <para>
      <userinput>PE <replaceable>event-num</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>event-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the purged event.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      Received upon completion of a one-shot event by
      <command>rdcatchd</command><manvolnum>8</manvolnum> to indicate that
      the event has been purged.
    </para>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.reload_time_offset">
    <title>Reload Time Offset</title>
    <para>
      Reload the time offset value from the database.
    </para>
    <para>
      <userinput>RO!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.reload_heartbeat_configuration">
    <title>Reload Heartbeat Configuration</title>
    <para>
      Reload the heartbeat configuration from the database.
    </para>
    <para>
      <userinput>RH!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.heartbeat_pulse">
    <title>Heartbeat Pulse</title>
    <para>
      Heartbeat Pulse, for connection keep-alive.
    </para>
    <para>
      <userinput>HB!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.restart_dropbox_instances">
    <title>Restart Dropbox Instances</title>
    <para>
      Restart all <command>rdimport</command><manvolnum>1</manvolnum>
      instances for running dropboxes.
    </para>
    <para>
      <userinput>RX!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.input_monitor_state">
    <title>Input Monitor State</title>
    <para>
      Turn the input monitor on or off.
    </para>
    <para>
      <userinput>MN <replaceable>deck-num</replaceable>
      <replaceable>state</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>deck-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the deck.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>state</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = Enabled,
	    <computeroutput>0</computeroutput> = Disabled.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="sect.privileged_commands.set_exit_code">
    <title>Set Exit Code</title>
    <para>
      Set the exit code of an event.
    </para>
    <para>
      <userinput>SC <replaceable>event-num</replaceable>
      <replaceable>code</replaceable>
      <replaceable>msg</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>event-num</replaceable></term>
	<listitem>
	  <para>
	    The number of the event.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>code</replaceable></term>
	<listitem>
	  <para>
	    The numeric code to set.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>msg</replaceable></term>
	<listitem>
	  <para>
	    The text message to set.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>



</sect1>

</article>
