B.30. Sierra Automated Systems 16000(D) Audio Router
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.30. Sierra Automated Systems 16000(D) Audio Router

Driver Name:

  SAS 16000(D)

Supported RML Commands:

  Switch Take ['ST']

Both analog and AES3 digital (D) variants are supported. Control can done by means of an RS-232C connection to the 'User Serial Interface' port on the unit. Serial port parameters should be: 9600,N,8,1.

Prev | Up | Next
B.29. Serial Port Modem Control Lines | Home | B.31. Sierra Automated Systems 32000 Audio Router