B.27. Quartz Electronics Type 1 Routing Protocol
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.27. Quartz Electronics Type 1 Routing Protocol

Driver Name:

  Quartz Type 1

Supported RML Commands:

  Fire Salvo ['FS']
  Switch Take ['ST']

Control can done either by means of an RS-232C connection or by means of TCP/IP to TCP port 23.

Prev | Up | Next
B.26. Modbus TCP | Home | B.28. Ross NK Video Switchers (via SCP/A Serial Interface)