Appendix B. Supported GPIO/Switcher Devices
Prev | Part III. | Next

## Appendix B. Supported GPIO/Switcher Devices

The following GPIO/switcher devices are supported under Rivendell:

## B.1. 360 Systems AM-16/B Audio Crosspoint Switcher

Driver Name:

  360 Systems AM-16/B

Supported RML Commands:

  Switch Take ['ST']

Control is done by means of MIDI connections to the 'MIDI IN' and 'MIDI OUT' ports on the back of the unit, with the appropriate MIDI device specified in the `Device:` field in `RDAdmin->ManageHosts->Switchers/GPIO`. The following settings should be configured on the AM-16/B:

Control Port Type:

  MIDI (jumper JMP1)

Program Send:

  OFF

Receive Channel: o

  o (Omni mode)

Memory Protect:

  OFF

The driver uses MIDI programs '0' and '1' on the AM-16/B when processing crosspoint changes; anything previously saved in those programs will be overwritten!

Prev | Up | Next
A.2. How to Apply These Terms to Your New Programs | Home | B.2. BroadcastTools 10x1