B.35. Sine Systems ACU-1 (Prophet Version)
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.35. Sine Systems ACU-1 (Prophet Version)

Driver Name:

  Sine ACU-1 (Prophet)

Supported RML Commands:

  Switch Add ['SA']
  Switch Remove ['SR']
  Switch Take ['ST']

Control is done by means of an RS-232C connection to the RS-232 port on the unit. Serial port parameters in RDAdmin should be set to 57600 baud rate, even parity, 8 data bits, 1 stop bit and no terminator.

The ACU-1 should be set to use factory default settings. This can be done by simultaneously pressing buttons 1 and 8 on the front panel of the unit for at least one second.

Prev | Up | Next
B.34. Sierra Automated Systems User Serial Interface (USI) | Home | B.36. Software Authority Protocol