<?xml version="1.0" encoding="ISO-8859-1"?>
<article xmlns="http://docbook.org/ns/docbook" version="5.0">
<info>
  <title>Rivendell Interprocess Communication Protocol</title>
  <author>
    <personname>
      <firstname>Fred</firstname>
      <surname>Gleason</surname>
      <email>fredg@paravelsystems.com</email>
    </personname>
  </author>
</info>

<sect1 xml:id="overview">
  <title>Overview</title>
  <para>
    This defines the IP protocol used for communication between different
    modules of Rivendell and the
    <command>ripcd</command><manvolnum>8</manvolnum> daemon.
  </para>
  <para>
    Connection to ripcd is by means of a TCP SOCK_STREAM connection to TCP
    port <userinput>5006</userinput>. The format of a message is as follows:
  </para>
  <para>
    <replaceable>cmd-code</replaceable> [<replaceable>arg</replaceable>] [<replaceable>...</replaceable>]!
  </para>
  <variablelist>
    <varlistentry>
      <term>
	<replaceable>cmd-code</replaceable>
      </term>
      <listitem>
	<para>
	  A two letter command code, describing the generic action to be
	  performed
	</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term>
	<replaceable>arg</replaceable>
      </term>
      <listitem>
	<para>
	  Zero or more arguments, delimited by spaces or, if the last
	  argument, by ! (see below)
	</para>
      </listitem>
    </varlistentry>
    <varlistentry>
      <term>
	!
      </term>
      <listitem>
	<para>
	  The ASCII character  33, indicating the end of the command sequence.
	</para>
      </listitem>
    </varlistentry>
  </variablelist>
</sect1>

<sect1 xml:id="sect.unprivileged_commands">
  <title>Unprivileged Commands</title>
  <para>
    No authentication is required to execute these.
  </para>
  <sect2 xml:id="sect.unprivileged_commands.drop_connection">
    <title>Drop Connection</title>
    <para>
      End the session and drop the TCP connection.
    </para>
    <para>
      <userinput>DC!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="sect.unprivileged_commands.send_password">
    <title>Send Password</title>
    <para>
      Send a password to the server for authentication.
    </para>
    <para>
      <userinput>PW <replaceable>passwd</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term>
	  <replaceable>passwd</replaceable>
	</term>
	<listitem>
	  A password to be supplied before granting the client access.
	</listitem>
      </varlistentry>
    </variablelist>
    <para>
      <command>ripcd</command><manvolnum>8</manvolnum> will respond
      with <computeroutput>PW +!</computeroutput> or
      <computeroutput>PW -!</computeroutput>, indicating the success or
      failure of the authentication.
    </para>
  </sect2>
</sect1>

<sect1 xml:id="sect.privileged_commands">
  <title>Privileged Commands</title>
  <para>
     A connection must be authenticated before these can be executed.
  </para>

  <sect2 xml:id="privileged_commands.request_user">
    <title>Request User</title>
    <para>
      Request the LOGIN_NAME of the user currently logged in.
    </para>
    <para>
      <userinput>RU!</userinput>
    </para>
    <para>
      <command>ripcd</command><manvolnum>8</manvolnum> will respond with
      <computeroutput>RU <replaceable>user-name</replaceable>!</computeroutput>.
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>user-name</replaceable></term>
	<listitem>
	  <para>
	    The LOGIN_NAME of the user currently logged in.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.set_user">
    <title>Set User</title>
    <para>
      Login in a user.
    </para>
    <para>
      <userinput>SU <replaceable>user-name</replaceable>!</userinput>
    </para>
    <para>
      <command>ripcd</command><manvolnum>8</manvolnum> will respond with
      <computeroutput>RU <replaceable>user-name</replaceable>!</computeroutput>.
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>user-name</replaceable></term>
	<listitem>
	  <para>
	    The LOGIN_NAME of the user to log in.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.rml_send">
    <title>RML Send</title>
    <para>
      Send an RML command to a specified host.
    </para>
    <para>
      <userinput>MS <replaceable>ip-addr</replaceable>
      <replaceable>echo</replaceable>
      <replaceable>rml</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>ip-addr</replaceable></term>
	<listitem>
	  <para>
	    IPv4 address of the destination, indotted-quad notation.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>echo</replaceable></term>
	<listitem>
	  <para>
	    <userinput>1</userinput> = Request echo,
	    <userinput>0</userinput> = Request no echo.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>rml</replaceable></term>
	<listitem>
	  <para>
	    The RML command to send.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.rml_echo">
    <title>RML Echo</title>
    <para>
      Echo an RML command to a specified host.
    </para>
    <para>
      <userinput>ME <replaceable>ip-addr</replaceable>
      <replaceable>echo</replaceable>
      <replaceable>rml</replaceable>!</userinput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>ip-addr</replaceable></term>
	<listitem>
	  <para>
	    IPv4 address of the destination, indotted-quad notation.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>echo</replaceable></term>
	<listitem>
	  <para>
	    <userinput>1</userinput> = Request echo,
	    <userinput>0</userinput> = Request no echo.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>rml</replaceable></term>
	<listitem>
	  <para>
	    The RML command to send.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.get_gpi_carts">
    <title>Get GPI Carts</title>
    <para>
      Return current GPI line cart numbers.
    </para>
    <para>
      <userinput>GC <replaceable>matrix</replaceable>!</userinput>
    </para>
    <para>
      Request the list of macro carts currently assigned for
      <replaceable>matrix</replaceable>. The following record will
      be returned for each line in the matrix:
    </para>
    <para>
      <computeroutput>GC
      <replaceable>matrix</replaceable>
      <replaceable>gpi-line</replaceable>
      <replaceable>off-cart-num</replaceable>
      <replaceable>on-cart-num</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>matrix</replaceable></term>
	<listitem>
	  <para>
	    The specified matrix number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>gpi-line</replaceable></term>
	<listitem>
	  <para>
	    The GPI line number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>off-cart-num</replaceable></term>
	<listitem>
	  <para>
	    The number for the cart to be activated when
	    <replaceable>gpi-line</replaceable> transitions to an OFF
	    state. <computeroutput>0</computeroutput> indicates that no
	    cart is currently set.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>on-cart-num</replaceable></term>
	<listitem>
	  <para>
	    The number for the cart to be activated when
	    <replaceable>gpi-line</replaceable> transitions to an ON
	    state. <computeroutput>0</computeroutput> indicates that no
	    cart is currently set.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.get_gpo_carts">
    <title>Get GPO Carts</title>
    <para>
      Return current GPO line cart numbers.
    </para>
    <para>
      <userinput>GD <replaceable>matrix</replaceable>!</userinput>
    </para>
    <para>
      Request the list of macro carts currently assigned for
      <replaceable>matrix</replaceable>. The following record will
      be returned for each line in the matrix:
    </para>
    <para>
      <computeroutput>GC
      <replaceable>matrix</replaceable>
      <replaceable>gpo-line</replaceable>
      <replaceable>off-cart-num</replaceable>
      <replaceable>on-cart-num</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>matrix</replaceable></term>
	<listitem>
	  <para>
	    The specified matrix number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>gpo-line</replaceable></term>
	<listitem>
	  <para>
	    The GPO line number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>off-cart-num</replaceable></term>
	<listitem>
	  <para>
	    The number for the cart to be activated when
	    <replaceable>gpo-line</replaceable> transitions to an OFF
	    state. <computeroutput>0</computeroutput> indicates that no
	    cart is currently set.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>on-cart-num</replaceable></term>
	<listitem>
	  <para>
	    The number for the cart to be activated when
	    <replaceable>gpo-line</replaceable> transitions to an ON
	    state. <computeroutput>0</computeroutput> indicates that no
	    cart is currently set.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.get_gpi_states">
    <title>Get GPI States</title>
    <para>
      Return current GPI states.
    </para>
    <para>
      <userinput>GI <replaceable>matrix</replaceable>!</userinput>
    </para>
    <para>
      Request the list of current GPI states for
      <replaceable>matrix</replaceable>. The following record will
      be returned for each line in the matrix:
    </para>
    <para>
      <computeroutput>GI
      <replaceable>matrix</replaceable>
      <replaceable>gpi-line</replaceable>
      <replaceable>state</replaceable>
      <replaceable>mask</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>matrix</replaceable></term>
	<listitem>
	  <para>
	    The specified matrix number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>gpi-line</replaceable></term>
	<listitem>
	  <para>
	    The GPI line number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>state</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = GPI is ON,
	    <computeroutput>0</computeroutput> = GPI is OFF.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>mask</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = GPI is ENABLED,
	    <computeroutput>0</computeroutput> = GPI is DISABLED.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.get_gpo_states">
    <title>Get GPO States</title>
    <para>
      Return current GPO states.
    </para>
    <para>
      <userinput>GO <replaceable>matrix</replaceable>!</userinput>
    </para>
    <para>
      Request the list of current GPO states for
      <replaceable>matrix</replaceable>. The following record will
      be returned for each line in the matrix:
    </para>
    <para>
      <computeroutput>GI
      <replaceable>matrix</replaceable>
      <replaceable>gpo-line</replaceable>
      <replaceable>state</replaceable>
      <replaceable>mask</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>matrix</replaceable></term>
	<listitem>
	  <para>
	    The specified matrix number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>gpo-line</replaceable></term>
	<listitem>
	  <para>
	    The GPO line number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>state</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = GPO is ON,
	    <computeroutput>0</computeroutput> = GPO is OFF.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>mask</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = GPO is ENABLED,
	    <computeroutput>0</computeroutput> = GPO is DISABLED.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.get_gpi_mask_states">
    <title>Get GPI Mask States</title>
    <para>
      Return current GPI mask states.
    </para>
    <para>
      <userinput>GM <replaceable>matrix</replaceable>!</userinput>
    </para>
    <para>
      Request the list of current GPI mask states for
      <replaceable>matrix</replaceable>. The following record will
      be returned for each line in the matrix:
    </para>
    <para>
      <computeroutput>GI
      <replaceable>matrix</replaceable>
      <replaceable>gpi-line</replaceable>
      <replaceable>mask</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>matrix</replaceable></term>
	<listitem>
	  <para>
	    The specified matrix number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>gpi-line</replaceable></term>
	<listitem>
	  <para>
	    The GPI line number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>mask</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = GPI is ENABLED,
	    <computeroutput>0</computeroutput> = GPI is DISABLED.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.get_gpo_mask_states">
    <title>Get GPO Mask States</title>
    <para>
      Return current GPO mask states.
    </para>
    <para>
      <userinput>GM <replaceable>matrix</replaceable>!</userinput>
    </para>
    <para>
      Request the list of current GPO mask states for
      <replaceable>matrix</replaceable>. The following record will
      be returned for each line in the matrix:
    </para>
    <para>
      <computeroutput>GN
      <replaceable>matrix</replaceable>
      <replaceable>gpo-line</replaceable>
      <replaceable>mask</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>matrix</replaceable></term>
	<listitem>
	  <para>
	    The specified matrix number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>gpo-line</replaceable></term>
	<listitem>
	  <para>
	    The GPO line number.
	  </para>
	</listitem>
      </varlistentry>
      <varlistentry>
	<term><replaceable>mask</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = GPO is ENABLED,
	    <computeroutput>0</computeroutput> = GPO is DISABLED.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

  <sect2 xml:id="privileged_commands.reload_gpi_table">
    <title>Reload GPI Table</title>
    <para>
      Reload the GPI table in <command>ripcd</command><manvolnum>8</manvolnum>.
    </para>
    <para>
      <userinput>RG!</userinput>
    </para>
  </sect2>

  <sect2 xml:id="privileged_commands.get_onair_flag">
    <title>Get OnAir Flag</title>
    <para>
      Request the state of the OnAir flag.
    </para>
    <para>
      <userinput>TA!</userinput>
    </para>
    <para>
      The following record will be returned:
    </para>
    <para>
      <computeroutput>TA<replaceable>state</replaceable>!</computeroutput>
    </para>
    <variablelist>
      <varlistentry>
	<term><replaceable>state</replaceable></term>
	<listitem>
	  <para>
	    <computeroutput>1</computeroutput> = Active,
	    <computeroutput>0</computeroutput> = Disabled.
	  </para>
	</listitem>
      </varlistentry>
    </variablelist>
  </sect2>

</sect1>

</article>
