B.10. BroadcastTools SRC-16
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.10. BroadcastTools SRC-16

Driver Name:

  BroadcastTools SRC-16

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']

Control is done by means of a serial connection to the unit's integrated serial port.

The unit should work correctly with factory default settings. The Rivendell serial interface should be set to use 9600 bits/sec, 8 bits, 1 stop bit and no flow control.

Prev | Up | Next
B.9. BroadcastTools Sentinel 4 Web AES Switcher | Home | B.11. BroadcastTools SS 12.4