B.22. Livewire Multicast GPIO
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.22. Livewire Multicast GPIO

Driver Name:

  Livewire Multicast GPIO

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']
  GPO Set ['GO']

Livewire is a distributed audio router and control system, with the components (called 'nodes') configured and controled via TCP/IP. More information can be found at http://www.axiaaudio.com/.

This driver provides the ability to access GPIO functions from Livewire- enabled control surfaces for setups that lack a virtual GPIO device --e.g. when interfacing audio directly to a Livewire node without using a native Livewire software audio driver or audio adapter.

When configuring it, the `IP Address` field should contain the address of the local interface to which the Livewire network is attached, while the `Livewire GPIOs` list should be populated with the stream number - GPIO line associations to be used.

Prev | Up | Next
B.21. Livewire LWRP GPIO | Home | B.23. Local Audio Adapter