B.23. Local Audio Adapter
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.23. Local Audio Adapter

Driver Name:

  Local Audio Adapter

Supported RML Commands:

  Switch Add ['SA']
  Switch Add With Gain ['SX']
  Switch Remove ['SR']
  Switch Take ['ST']

It's possible to use one or more of the actual audio adapters as a switcher device using this driver. Doing so makes it possible to route audio directly from the adapter inputs to outputs, while at the same time using it for audio capture/playout in the usual manner.

To configure it, set `Card:` to the number of the audio adapter to use and the `Inputs:` and `Outputs:` fields to the number of inputs and outputs on the card (as found in `RDADmin->ManageHosts->AudioResources`.

Prev | Up | Next
B.22. Livewire Multicast GPIO | Home | B.24. Local GPIO