B.17. BroadcastTools Universal 4.1MLR>>Web
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.17. BroadcastTools Universal 4.1MLR>>Web

Driver Name:

  BroadcastTools 4.1 MLR>>Web

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']
  Switch Take ['ST']

Control is by means of a TCP/IP connection to port 5002.

Prev | Up | Next
B.16. BroadcastTools SS8.2 | Home | B.18. Harlond Virtual Mixer