B.34. Sierra Automated Systems 64000 Audio Router
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.34. Sierra Automated Systems 64000 Audio Router

Driver Name:

  SAS 64000-GPI

Supported RML Commands:

  GPO Set ['GO']
  Switch Take ['ST']

Control is done by means of an RS-232C connection to the 'Computer RS-232' port on a GPI-1600 GPIO interface. Serial port parameters should be set to 19200 baud rate, no parity, 8 data bits, 1 stop bit and no terminator. This driver allows control of the system's GPO outputs as well as audio crosspoints.

Prev | Up | Next
B.33. Sierra Automated Systems 64000 Audio Router | Home | B.35. Sierra Automated Systems User Serial Interface (USI)