B.27. Modbus TCP
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.27. Modbus TCP

Driver Name:

  Modbus TCP

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']
  GPO Set ['GO']

This driver supports GPI devices that use the industry-standard Modbus TCP protocol at TCP port 502. The device to be controlled should be configured to use Modbus ID #1. For more information on Modbus, see http://www.modbus.org/.

Prev | Up | Next
B.26. Logitek vGuest | Home | B.28. Quartz Electronics Type 1 Routing Protocol