B.24. Local Audio Adapter
Prev | Appendix B. Supported GPIO/Switcher Devices | Next

## B.24. Local Audio Adapter

Driver Name:

  Local Audio Adapter

Supported RML Commands:

  GPI Enable ['GE']
  GPI Set ['GI']
  GPO Set ['GO']
  Switch Add ['SA']
  Switch Add With Gain ['SX']
  Switch Remove ['SR']
  Switch Take ['ST']

It's possible to use one or more of the actual audio adapters as a switcher device using this driver. Doing so makes it possible to route audio directly from the adapter inputs to outputs, while at the same time using it for audio capture/playout in the usual manner.

To configure it, set `Card:` to the number of the audio adapter to use and the `Inputs:` and `Outputs:` fields to the number of inputs and outputs on the card (as found in `RDADmin->ManageHosts->AudioResources`).

For AudioScience cards that include onboard GPIO (such as the ASI67xx series), the GPIO resources on the card will also be available via the this driver.

Prev | Up | Next
B.23. Livewire Multicast GPIO | Home | B.25. Local GPIO